Current Help System: PC-DMIS Laser (View Core Help)

#### CMS Sensors

Laser Sensor tab for the CMS probe

1. Use the IP address and Port # boxes to define the IP address and of the CMS controller.

2. If desired, use the Beep level box to set the volume for beep sounds coming out of the CMS controller. It can accept any value from 0 to 100. 0 turns off the volume completely.

The Laser Sensor tab also displays the installed CMS Toolkit version.