Current Help System: PC-DMIS Laser (View Core Help)

#### Analysis Area

The Analysis area allows you to determine how each measured hit/point is displayed.

Pt. Size: Determines how big the measured points will be drawn in the Cad View. This value specifies the diameter, as is specified in current units (mm or inch).

Graphic Analysis button : When switched on, PC-DMIS will do a tolerance check on each point (how far from theoretical position it is), and draw them in the appropriate based on the current defined dimension color range.

+ Tol: This provides the positive tolerance from the nominal, and is specified in current part program units. Points that are greater than this value from the nominal will be colored based on the standard PC-DMIS plus tolerance color. See the "Editing Dimension Colors" topic in the PC-DMIS Core help file.

- Tol: This provides the negative tolerance from the nominal, and is specified in current part program units. Points that are less than this value from the nominal will be colored based on the standard PC-DMIS negative tolerance color. See the "Editing Dimension Colors" topic in the PC-DMIS Core help file.