Current Help System: PC-DMIS Laser (View Core Help)

## Using Sound Events

Sound Events provide audible feedback in addition to the visual user interface. This allows you to perform measuring actions without needed to look at the PC screen. To access the Sound Events tab of the SetUp Options dialog box, select the Edit | Preferences | Setup menu item.

When working with a laser device there are Sound Event options that are particularly useful. They are:

Laser Manual Calibration Bottom: This sound is played when calibration measurements for a given field should be taken in the upper region of the sphere.

Laser Manual Calibration Field Counter: This sound is played to indicate in which field measurements should be taken during calibration.

- 1 Beep - Far

- 2 Beeps - Left

- 3 Beeps - Right

Laser Manual Calibration Top: This sound is played when calibration measurements for a given field should be taken in the lower region of the sphere.

Laser Probe Initialization End: This sound is played when at the end of the laser sensor initialization.

Laser Probe Initialization Start: This sound is played when at the beginning of the laser sensor initialization.

Laser Scan: This sound is played for each new step of the sensor calibration.