Current Help System: PC-DMIS Laser (View Core Help)

### Step 5: Check the Calibration Results

Click on the Results button in the Probe Utilities dialog box. The Calibration Results dialog box appears.

Calibration Results

PC-DMIS records several things from the calibration in this dialog box. Take a look at the maximum, average, and standard deviation values.

The maximum should be somewhere between 20 to 100 microns. The average and the standard deviation should be around 20 microns.

If things look correct, click the OK button to close down the Calibration Results dialog box.

You are now done setting up and calibrating your laser probe. You should now have access to all laser-related functionality.