Current Help System: PC-DMIS Laser (View Core Help)

#### Sensitivity (for CMS Sensors)

Sensitivity list

CMS sensors provide you with an additional list called Sensitivity which is added onto the Laser Scan Properties tab of the Probe Toolbox. This lets you choose between two sensitivity modes:

- HIGH sensitivity - This makes the sensor much more sensitive.

- NORMAL sensitivity - This is the default sensor mode and should be used on most normal parts.

Important: You should only use the HIGH sensitivity mode if you are scanning a part comprised of a troublesome material where the NORMAL sensitivity mode returns poor data. For example, a part that absorbs too much light because it has dark or black surfaces may require this type of mode. Be aware that scanning a normal part in HIGH sensitivity mode may yield bad results.