Current Help System: PC-DMIS Portable (View Core Help)

### Step 3: Launch PC-DMIS and Configure the Leica Interface

Once you have correctly installed PC-DMIS and connected your Leica tracker, you are ready to launch PC-DMIS.

1. Start PC-DMIS using the shortcut you created in Step 1. The Leica Tracker will initialize upon PC-DMIS startup. Initialization will cause the tracker to go through a series of movements to ensure proper functionality. If there are other issues that cause the Leica Tracker to not initialize correctly, the LT controller will send messages to PC-DMIS for display.

2. PC-DMIS will warn you if the laser is still warming up (this takes about 20 minutes).

3. Select the needed probe file from the Select Probe File dialog box.

4. "Configure the Leica Interface" using Machine Options dialog box that is accessed using the Edit | Machine Interface Setup menu item.

Next Step...