Current Help System: PC-DMIS Portable (View Core Help)

### Tracker Status Bar

Tracker Status bar visibility can be toggled using the View | Statusbar | Tracker menu item.

1. System Laser Status Indicator: This indicates the status of the Laser Tracker system.

- Green (Ready): The system is ready to measure

- Yellow (Busy): The system is currently measuring

- Red (Not ready): The system is not ready to measure. This may be due to a broken beam or a T-Probe reflector mismatch.

- Blue (6dof error): The camera cannot see enough LED’s on the device (usually T-Probe) to accurately calculate the orientation of the probe.

2. Active Station Indicator: Indicates which station is currently active. A double click onto the station Indicator opens the Station Manager dialog box.

- Red (Not oriented): The station position is not computed yet.

- Green (Oriented) The station position has been computed.

3. Environmental Parameter Display: Shows the active environmental parameters: temperature, pressure, and humidity. If no weather station is connected, it is possible to double-click on the edit boxes to change their values.