Current Help System: PC-DMIS Settings Editor (View Core Help)

### ACR2 Calibrate

Allows specification of a Prehit distance in mm, Depth along the pin axis for the measured circle in mm and probing Speed to be used during calibration of an ACR2 probe change rack when it measures the pin inside the port to determine the location. You should not normally need to modify these values.

Entry Name: ACR2_Calibrate

Entry Type: Character String specifying ACR2 calibration values Default value is “Prehit=-4 Depth=0 Speed=-1”.

User permission is required to change entry