Current Help System: PC-DMIS Settings Editor (View Core Help)

### Cmm Calibrated As Slave

This value is used to tell PC-DMIS that the attached CMM has been calibrated as a slave in a dual arm configuration. The slave computer relays commands from the master computer.

Entry Name: CmmCalibratedAsSlave

Entry Type: Whole Number specifying CMM status. Default value is 0.

User permission is required to change entry