Current Help System: PC-DMIS Settings Editor (View Core Help)

### Round Slot CG Gray Sum Min

Provides the minimum pixel intensity below which pixels exceeding this value will not be used. This value is used when measuring laser round slot features using the Gray Sum locater type.

Entry Name: RoundSlot_CGGraySumMin

Entry Type: Whole Number specifying minimum pixel intensity. Default value is 50.

User permission is required to change entry