Current Help System: PC-DMIS Settings Editor (View Core Help)

### Illumination Off For Contact Probe

This entry controls whether or not lamps remain turned on when the part program switches from a vision probe to a contact probe.

Entry Name: IlluminationOffForContactProbe

Entry Type: Boolean. Setting this to TRUE causes the lamps to be turned off when switching to a contact probe. Setting it to FALSE will keep the lamps turned on. The default is FALSE.

User permission is required to change entry