Current Help System: PC-DMIS Settings Editor (View Core Help)

### Cylinder CG Gray Sum Max

Provides the maximum pixel intensity beyond which pixels exceeding this value will not be used. This value is used when measuring laser cylinder features using the Gray Sum locater type.

Entry Name: Cylinder_CGGraySumMax

Entry Type: Whole Number specifying maximum pixel intensity. Default value is 300.

User permission is required to change entry