Current Help System: PC-DMIS Settings Editor (View Core Help)

### Head Collision Check Distance

Specifies the overhang in Y axis of the probe head as measured from the center of the gripper pins to the end of the probe head. You may need to manually measure the length of the probe to get this value.

Entry Name: HeadCollisionCheckDistance

Entry Type: Real Number to specify check distance. Default value is 270.

User permission is required to change entry