Current Help System: PC-DMIS Settings Editor (View Core Help)

### Conical Tolerance

Determines the conical tolerance for added Tip changes. This allows PC-DMIS to utilize a tip that has a shank vector that is within the tolerance of the optimal vector angle for a given feature.

Entry Name: ConicalTolerance

Entry Type: Real Number to specify an angle. Default value is 5.

User permission is required to change entry

For features such as points, lines, and planes there is a built in conical range of 90 degrees since a plane with a vector of 0, 0, 1 could be measured by T1A0B0 or T1A90B0. In the case of these features, PC-DMIS adds the user entered value to the built-in range. The proposed tip angle is also checked by running collision detection (silently) to determine if the tip will actually work.