Current Help System: PC-DMIS Settings Editor (View Core Help)

### Wrist C Angle Increment

Provides the angle increment between the starting and ending C angles. Angles will be calibrated for your wrist device for the starting, ending, and additional angles as determined by the increment value. For example, an increment angle of 10 degrees would add angles for calibration every 10 degrees between the starting and ending angle.

Entry Name: WristCAngleIncrement

Entry Type: Real Number to specify C angle increment. Default value is 10.

User permission is required to change entry