Current Help System: PC-DMIS Settings Editor (View Core Help)

### Temp Comp Automatic

This option determines the method that will be used for Temperature Compensation.

Entry Name: TempCompAutomatic

Entry Type: Whole Number to specify the Compensation Method. Default value is 0.

User permission is required to change entry

The following are the available compensation methods and their respective processes in PC-DMIS.

Value | Method | Process
0 | Manual | Compensation is manual.
1 | Read Temperatures from Controller | PC-DMIS reads the current temperatures from the controller automatically rather than you supplying the data.
2 | Controller Compensates Axes Only | The controller performs compensation of the machine axes itself.
3 | Controller Comps Axes and Part | The controller performs compensation of both the machine axes and the part.