Current Help System: PC-DMIS Settings Editor (View Core Help)

### External Rotab Status Auto Retries

Provides the number of times a status request should automatically be retried in the event of a timeout before the user is prompted. This always applies to the status timeout and may apply to the init timeout if it was a status command that timed out on the initial communication attempt. It specifically does not apply to a move timeout or stop timeout. Resending of commands that initiate or terminate table motion must be explicitly confirmed by the user.

Entry Name: ExternalRotabStatusAutoRetries

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 1.

User permission is required to change entry