Current Help System: PC-DMIS Settings Editor (View Core Help)

### Rotary Polar

Rotary scans allow you to define boundary points using Polar coordinates rather than Cartesian coordinates. Values are then given in Radius, Angle, and Height. Polar coordinates are used when this value is set to TRUE (1).

Entry Name: RotaryPolar

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry