Current Help System: PC-DMIS Settings Editor (View Core Help)

### Animated Machine Arm Overlap

Provides the machine arm overlap for the display of dual arm configurations in the Graphics Display Window. The provided value will overlap the two measuring volumes by this value. Both positive and negative values can be used. Negative values create a gap of the specified distance between the two measuring volumes.

Entry Name: AnimatedMachineArmOverlap

Entry Type: Real Number specifying overlap distance in MM. Default value is 100.

User permission is required to change entry