Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Optics Cal Focus Latency Duration 2

Provides the duration in seconds of the low speed focus latency calibration scan.

Note: For optimal calibration results this values should be as small as practical and the difference between this value and "ProbeQualVisionOpticsCalFocusLatencyDuration1" should be large.

Entry Name: ProbeQualVisionOpticsCalFocusLatencyDuration2

Entry Type: Real Number specifying time in seconds. The default is 8.

User permission is required to change entry