Current Help System: PC-DMIS Settings Editor (View Core Help)

### Light Model 2 Side

This option determines whether or not the front and back faces of surfaces should be lighted. You should select this check box for imported IGES files, and for some other CAD formats when the surface normals are not correct.

Entry Name: LightModel_2Side

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.

User permission is required to change entry