Current Help System: PC-DMIS Settings Editor (View Core Help)

### Ref Temp (PXYZ)

The Ref Temp values contain the reference temperature from which temperature compensation adjustments need to be applied.

- The amount of correction to be applied is based on multiplying the material coefficient by the difference between the current and reference temperatures.
  Amount of Correction = Material Coefficient x (Current Temp – Reference Temp)

- If the current temperature is the same as the reference temperature the net effect is that no thermal compensation adjustment is applied.

Entry Name: RefTemp(PXYZ)

Entry Type: Character String specifying degrees in either Celsius or Fahrenheit. Default value is None ( ).

User permission is required to change entry

Option Key:

X | X Axis
Y | Y Axis
Z | Z Axis
P | Part