Current Help System: PC-DMIS Settings Editor (View Core Help)

### CG Threshold

This value is used when the "SensorCGLocType" value is set to 1 (Fixed Threshold). See the "Laser Probe Toolbox: Laser Pixel Locator Properties tab" topic in the PC-DMIS Laser documentation for more information. PC-DMIS discards all the data below the threshold and it computes the actual pixel location as the center of gravity of the remaining pixels within the column.

Entry Name: CGThreshold

Entry Type: Whole Number specifying threshold in pixels. Default value is 0.

User permission is required to change entry