Current Help System: PC-DMIS Settings Editor (View Core Help)

### Screen Capture Time

Determines when an image will be captured for the SCREENCAPTURE.RTP for Laser or Vision Auto Features. The "ScreenCaptureQuality", "ScreenCaptureScale" and "ScreenCaptureType" values are also used to determine the properties of the captured image.

Entry Name: ScreenCaptureTime

Entry Type: Whole Number to specify criteria for capturing screen captures. Default value is 0.

User permission is required to change entry

Value Key:

0 | ALL | Image capture gets generated for ALL measurements of this feature. Please be aware that this may cause your reports to become too big.
1 | FAILED | Image capture gets generated only when any point section that includes at least one point that exceeded your specified "PointToleranceMinus" and "PointTolerancePlus" values.