Current Help System: PC-DMIS Settings Editor (View Core Help)

### Uv Scan Cutoff Factor

This value is used when importing Inspection Plans through the AIMS DCI. This option uses a positive numeric value to help determine what type of scan will be created from a surface feature. The default value is 3. Larger values will cause UV scans to be favored. Lower values will favor freeform scans.

Entry Name: UvScanCutoffFactor

Entry Type: Real Number to specify the cutoff factor. Default value is 3.

User permission is required to change entry