Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Optics Cal Rotation Line Y Offset

Provides the distance from the center of the optics calibration grid to the horizontal line on the bottom of the optical slide that is used to calibrate the rotation.

Entry Name: ProbeQualVisionOpticsCalRotationLineYOffset

Entry Type: Real Number to specify distance in pixels. Default value is 20.

User permission is required to change entry