Current Help System: PC-DMIS Settings Editor (View Core Help)

### Body Axis Scan Axis

Specifies the axis to be used with Body Axis scans. The available axes are X, Y, and Z. The cut plane that your probe will crisscross will be parallel to this axis.

Entry Name: BodyAxisScanAxis

Entry Type: Whole Number specifying axis number. Default value is 0.

User permission is required to change entry

Axis Key

0 | X
1 | Y
2 | Z