Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Snap

Determines whether the "Snap Point" option will be used when creating a Surface Point or Vector Point auto feature. When this option is set to TRUE (1), the measured values "snap to" the theoretical vector when a supported feature is measured. All the deviation will be along the vector of the point. This is useful for focusing on a deviation along one particular vector.

Entry Name: DCCSnap

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry

See the "Snap List" topic in the core PC-DMIS documentation.