Current Help System: PC-DMIS Settings Editor (View Core Help)

### Collision Tolerance in MM

Provides a buffer zone around the probe and tip geometry so that PC-DMIS considers close misses as collisions. This value is adjusted for geometry that is below the trigger using the "BelowTriggerTolerancePercentage" value.

Entry Name: CollisionTolleranceInMM

Entry Type: Real Number to specify distance in MM. Default value is 0.

User permission is required to change entry