Current Help System: PC-DMIS Settings Editor (View Core Help)

### Optimize Adjust Theo Thickness

Optimize Path has a routine that automatically determines thickness type by flipping vectors as needed to accommodate differences between measured feature vectors and CAD vectors.

When no thickness is reported from CAD, and Optimize Path does not flip the vector, then the thickness type would be set to 'none'. However if Optimize Path does flip the vector, then thickness type is set to 'theoretical' for Chrysler, and 'actual' for AUDI.

When this value is set to TRUE (1), then the thickness type is set to 'actual' when Optimize Path flips the vector. Otherwise, when set to FALSE (0), then the thickness type is set to 'theoretical'.

Entry Name: OptimizeAdjustTheoThickness

Entry Type: True/False value. Default value is FALSE.

User permission is required to change entry