Current Help System: PC-DMIS Settings Editor (View Core Help)

### CMT IP Address

Provides the TCPIP Address of your NC-100 computer system. This value is required for the communication between the PC-DMIS computer system and the NC-100 computer system.

Entry Name: CMTIPAddress

Entry Type: Character String to specify TCP/IP Address. Default value is 0.0.0.0.

User permission is required to change entry