Current Help System: PC-DMIS Settings Editor (View Core Help)

### Focus Surface Variance MM

When "FocusFindSurface" is set to TRUE, this value is used to determine how far PC-DMIS will search for the focal position. Once the focal position is found, PC-DMIS will do a quick focus scan in that region.

Entry Name: FocusSurfaceVarianceMM

Entry Type: Real Number specifying distance in pixels. The default is 5.

User permission is required to change entry