Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Targ XYZ _2

Provides the default "Z" or "H" (height) value for the center location for all auto features created with the NC-100 video probe. The value will represent Z value when the "Cartesian" value is set to TRUE (1), and H when it is set to FALSE (0).

Entry Name: DccTargXYZ_2

Entry Type: Real Number to specify the Z or H value. Default value is 0.

User permission is required to change entry