Current Help System: PC-DMIS Settings Editor (View Core Help)

### Valisys Comm Port

Specifies the COM port that is used to establish a serial connection between your PC-DMIS computer and your Valisys server. Use a value of 1 for COM1, 2 for COM2, etc. The protocol for the port will automatically be set to 9600 baud, 8 data bits, no parity, 1 stop bit. The Valisys host must be configured to use the same settings protocol settings.

Note: When a serial port is being used there should not be an entry for ValisysTCPIPPort.

Entry Name: ValisysCommPort

Entry Type: Whole Number to specify the COM port. Default value is 0

User permission is required to change entry