Current Help System: PC-DMIS Settings Editor (View Core Help)

### Dimension 132 Columns

This option controls the printing format of feature locations in the inspection report. When this value is set to TRUE (1), PC-DMIS will print all feature locations in a 132 column format.

Entry Name: Dimension132Columns

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry

The following describes the columns in the 132 column printout format:

Column 1 to 10:X nominal
Column 11 to 20:X measured
Column 21 to 28:X deviation
Column 31 to 40:Y nominal
Column 41 to 50:Y measured
Column 51 to 58:Y deviation
Column 61 to 70:Z nominal
Column 71 to 80:Z measured
Column 81 to 88:Z deviation
Column 91 to 100T error (normal to surface error)
Column 101 to 101Out of Tol flag "*"
Column 104 to 105Feature type
Column 108 to 117Feature ID
Column 118 to 127Measured Diameter if any