### Adjust Find Hole By Last Hit

This option should be set to FALSE, if there is the risk to contact the edge of the feature with the stem of the tip.

Entry Name: AdjustFindHoleByLastHit

Entry Type: True/False value. Default value is FALSE.

User permission is required to change entry

This might be a problem when Tip angle is different from the vector of the feature because the wrist (TESA for instance), has at least a resolution of 5 degrees as shown below.

If the vector of the tip is sufficiently parallel to the vector of the feature, then it will always touch the ball and not the stem.