Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Filter Type

This is used for persistent storage of the default value of the Laser filter as described in the Laser Documentation. See the "Laser Probe Toolbox: Laser Filtering Properties tab" topic in the PC-DMIS Laser documentation for more information.

Entry Name: SensorFilterType

Entry Type: Whole Number specifying filter type. Default value is 0.

User permission is required to change entry

Filter Type Key:

0 | None
1 | Long Line
2 | Median
3 | Inline
4 | Weighted Average