Current Help System: PC-DMIS Settings Editor (View Core Help)

### Screen Capture Quality

Determines the Quality that will be used for Screen Capture images that are included in the SCREENCAPTURE.RTP for Laser or Vision Auto Features. The "ScreenCaptureScale", "ScreenCaptureTime" and "ScreenCaptureType" values are also used to determine the properties of the captured image.

Entry Name: ScreenCaptureQuality

Entry Type: Whole Number to specify quality option. Default value is 0.

User permission is required to change entry

Value Key:

0 | Low | The color depth of the image is 2 bits per pixel resulting in a loss of color information on all but the simplest of images (e.g. where most pixels are black or white).
1 | Good | The color depth of the image is 4 bits per pixel, which gives acceptable images except where the image contains a lot of different colors, where a loss of color information is noticeable.
2 | High | The color depth of the image is 8 bits per pixel, which produces little to no color loss.