Current Help System: PC-DMIS Settings Editor (View Core Help)

### Gripper Mount (XYZ)

These three values define the XYZ location that is used for a Gripper Mount Point for the master arm. This is a position that the machine will move to when it is time to mount the gripper onto the end of the ram. To determine what these values should be, move the machine to the desired location where the probe is easy to reach. Enter the XYZ values to their respective registry values.

Entry Name: GripperMount(XYZ)

Entry Type: Real Number to specify (XYZ) gripper mount point location. Default value is -999999.

User permission is required to change entry