Current Help System: PC-DMIS Settings Editor (View Core Help)

### Wrist B Angle End

Provides the ending B angle used for the calibration of your wrist device. As part of the calibration process, you need to calibrate wrist positions in a pattern of at least three A angle positions by at least three B angle positions for a total of nine sphere measurements.

Entry Name: WristBAngleEnd

Entry Type: Real Number to specify the ending B angle. Default value is -180.

User permission is required to change entry