Current Help System: Tutor Translator (View Core Help)

## Motion Control

MANMOVE translates to è

MODE/MANUAL

NCMOVE translates to è

IF/GETSETTING("Dcc mode") == 1

C1 =COMMENT/YESNO,NO, ”Do you want continue in CNC mode?”

IF/C1.INPUT=="YES"
IF/GETSETTING("Current Alignment")=="STARTUP"
COMMENT/OPER,NO,TUTOR TRANSLATOR WARNING!
,Move and hits commands executed in STARTUP alignment could be ,affected by a probe offset error due to the difference in probe ,management between Tutor and PC-DMIS!
,Continue in safety mode or change moves and hits mode to RELEARN in order to relearn them!
END_IF/
MODE/DCC
END_IF/
END_IF/

NCMOVE NOCONF translates to è

MODE/DCC

The command FLY(ON) uses the length of the last value defined with FLY(ON,LENGTH=val). The default value is 30 mm. PC-DMIS does not allow FLY without a length parameter so a variable must defined at the beginning of the part program and initialized with:

- 30 mm if the PC-DMIS part program is in metric mode.

- 1.1811 inch if the PC-DMIS part program is in inch mode.

FLY(ON) translates to è

FLY/ON,E.FLYLEN

FLY(ON,LENGTH=23) translates to è

ASSIGN/E.FLYLEN = 23
FLY/ON,E.FLYLEN

FLY(OFF) translates to è

FLY/OFF,E.FLYLEN