Current Help System: Tutor Translator (View Core Help)

### Thickness Measurement Commands

MTHICHNS (MEMORY [10], 5) translates to è

ASSIGN/E.BADMEAS=0

PLN4 = FEAT/PLANE,RECT

THEO/<0.2502,350,0.2>,<1,0,0>
ACTL/<0.2502,350,0.2>,<1,0,0>
MEAS/PLANE,4
…
… move/hit/tip commands for plane PLN1
…
ENDMEAS/

PNT1 = FEAT/POINT,RECT

THEO/<23,340,0>,<0,0,1>
ACTL/<23,340,0>,<0,0,1>
MEAS/POINT,1
…
… move/hit/tip commands for point PNT1
…
ENDMEAS/

PNT2 = FEAT/POINT,RECT

THEO/<0.2502,340,0>,<1,0,0>
ACTL/<0.2502,340,0>,<1,0,0>
CONSTR/POINT,PROJ,PLN4,PNT1

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("PNT1")
ASSIGN/E.WM1.DS = DIST3D({PNT1},{PNT2})
ASSIGN/E.MEMORY[10] = E.WM1
…
… Evaluation commands.
…