Current Help System: Tutor Translator (View Core Help)

## Movement Parameters

In PC-DMIS the measure speed is limited to 20% of the max CMM speed. In contrast Tutor allows the measure speed to be set higher than 20% (up to 100%). If the measurement speed is higher than 20 then it is limited to 20 for PC-DMIS.

MSPEED 10 translates to è

TOUCHSPEED/10

MSPEED 80 translates to è

TOUCHSPEED/20
MSPEEDVAL = 50
. . . .

MSPEED MSPEEDVAL translates to è

ASSIGN/ E.MSPEEDVAL = 50
. . . .
TOUCHSPEED/ E.MSPEEDVAL

PSPEED 80 translates to è

MOVESPEED/80
PSPEEDVAL = 50
. . . .

PSPEED PSPEEDVAL translates to è

ASSIGN/ E.PSPEEDVAL = 50
. . . .
MOVESPEED/ E.PSPEEDVAL

The ACC command is translated as COMMENT/DOC command with the suggestion to use the PC-DMIS ACCELERATION command.

ACC 50 translates to è

COMMENT/DOC,NO,=======================================
,= ACC 50
,= Not translated command: Modify manually
,= Suggested command:
,= ACCELERATION/MAXACCELX=Xval, MAXACCELY=Yval,
,= MAXXACELZ=Zval
,=====================================================

DIST_APPROACH 12. translates to è

PREHIT / 12.
RETRACT / 12.

DIST_APPROACH , 12. translates to è

CHECK/ 12.

DIST_APPROACH 12. , 24. translates to è

PREHIT / 12.
RETRACT / 12.
CHECK/ 24.

The FEED and OPT_SPEED commands are not translated because they are not supported by PC-DMIS