Current Help System: Tutor Translator (View Core Help)

#### Tutor

1. There is no theoretical probe definition. If PH9 is present the Roll and Pitch values are required.

2. When calibrating the gauge, the tool offset (distance from RAM and the tip) must be supplied. Calibration also computes the dynamic tip radius of calibration probe.

3. The qualification procedure computes the probe offset (in respect to the Calibration probe) and the tip radius.

4. Movement and measured coordinates are computed without the tool offset. This could be a problem executing DCC movement using the machine reference system (STARTUP). The Tool offset is only used to properly compensate/decompensate the coordinates and hits.

5. Probes are identified by a couple of numbers (Head and Tip).

6. Probes file management command (Load/Save).

7. Calibration/Qualification commands.

8. No automatic Calibration/Qualification procedure.