Current Help System: PC-DMIS Vision (View Core Help)

#### Edge Point Field Definition with NC-100

This is already covered in the "Edge Point Field Definitions" topic in the "Creating Auto Features" section. The following is specific to NC-100 video probes:

ACTL_THICKNESS = This value indicates the keyed in offset thickness of the measured data. Positive or negative values can be used.

SHOWHITS = This is a toggle field. It toggles from YES to NO and determines if hits will be displayed with this feature. This is not currently available with Edge Points.

SHOWALLPARAMS = This is a toggle field. It toggles from YES to NO as to displaying all the parameters on an Edge Point

EDGE ACTL_THICKNESS = This value indicates the keyed in offset thickness of the measured edge. Positive or negative values can be used.

DEPTH = This value is an editable distances. (Only Available on “EDGE DELTAZ”)