Current Help System: PC-DMIS Vision (View Core Help)

#### Step 6: Calibrating All Needed Probe Tip Positions on the Sphere Tool

In this step you will be using the sphere calibration tool to measure the new positions added at the end of the previous step. It's best if you haven't moved the tool since you used it last.

1. Select the newly added tip positions from the Active Tip List of the Probe Utilities dialog box.

2. Click the Measure button. The Measure Probe dialog box appears.

3. Select the DCC or ManDCC option button.

4. Select the Calibrate Tips option button in the Type of Operation area.

5. Select the sphere calibration tool from the List of Available Tools list.

6. Click the Measure button. If the DCC option was selected, PC-DMIS will automatically begin to measure the sphere using the various probe tip positions.

7. After calibration, PC-DMIS returns to the Probe Utilities dialog box.

Next Step...