Current Help System: PC-DMIS Vision (View Core Help)

### Live View Alignments

This section describes the process of creating alignments using the Live View in PC-DMIS Vision. This is commonly used when you are measuring online but have not imported CAD. Creating both Manual (rough) and DCC (refined) alignments as outlined below will help ensure the accuracy of your alignment. This two-step alignment process is not required but is recommended.

If you are working on manual machine you can take advantage of this two-alignment approach by using the AutoShutter feature to assist you. See "Setting up the Live View" for information on the AutoShutter feature.

Complete the following steps to create an alignment using the Live View:

- Step 1: Manually Measure Datum Features

- Step 2: Create a Manual Alignment

- Step 3: Remeasure the Datum Features

- Step 4: Create a DCC Alignment

In this example the 3 2 1 Alignment Wizard will be used to show how this tool can be used, where the "Cad View Alignments" example will use the classic Alignment Utilities dialog box.