Current Help System: PC-DMIS Vision (View Core Help)

#### CMM-V Probe Offset

To calibrate a CMM-V probe offset, do the following:

1. Create a touch probe with all the angles at which measurements will be taken with your CMM-V vision probe.

Note: Your touch probe must be a star probe with at least 3 tips.

2. Calibrate all specified touch probe angles on a sphere.

3. Measure the A0B0 touch probe angle on a ring gage.

4. Measure the A0B0 video probe on the same ring gage, answering “No” when asked if the tool has moved.

5. Click Add Angles when you have the CMM-V probe selected. Rather than showing the standard Add Angles dialog, it will prompt you with a list of touch probes.

6. Select the touch probe you have calibrated on the sphere, and press OK. PC-DMIS Vision will automatically add those angles and calibrations to your CMM-V video probe.