PC-Dmis 2010 MR2 Object Library | Send comments on this topic. | See Object Hierarchy Chart
AlignCmnd Object Members
See Also Overview

Collapse All Expand All

# Public Methods

AddBestFitFeat | Adds best fit feature to BF3D or BF2D alignments
AddLevelFeat | Adds level feature to iterative alignment
AddOriginFeat | Adds origin feature to iterative alignment
AddRotateFeat | Adds rotation feature to iterative alignment
CalculateDeviation | Returns deviation value and vector for a feature
CalculateDeviation2 | Returns theoretical, measured and deviations of input after alignment values
CalculateMatrices | Forces immediate calculation of alignment matrices Forces the immediate calculation of alignment matrices.
CalculateStatistics | Returns the mean and standard deviation
GetBFIterations | Returns the number of bestfit iterations
GetFeatureIdByIndex | Returns the feature id

# Public Properties

AboutAxis | Read/Write: The axis about which alignment is rotated Represents the axis about which the alignment object rotates.
Angle | Read/Write: Point data object with angle values for BF3D and BF2D alignments Represents the offset angles of a 3D or 2D alignment.
AverageError | Read/Write: Average Error setting for Iterative Alignments Represents whether or not error averaging is used during the iterative alignment.
AXIS | Read/Write: The alignment axis Represents the axis that the alignment object uses.
BFOffset | Read/Write: Point data object with best fit offsets for BF3D and BF2D alignments Represents the offsets of a 3D or 2D alignment.
CadToPartMatrix | Read Only: Returns a DmisMatrix object representing the cad to part matrix for the alignment Represents the matrix used to transform points between the cad and part alignment systems.
ExternalFileID | Read/Write: External filename for recalling external alignments Represents the external filename for recalling external alignments.
ExternalID | Read/Write: ID of External Alignment Represents the external ID.
FeatID | Read/Write: Feature referenced by the alignment Represents the first (or only) feature ID used by this alignment object.
FeatID2 | Read/Write: Second referenced alignment feature Represents the second feature ID used by this alignment object.
FindCad | Read/Write: Find Cad setting for BF3D and BF2D alignments Represents the FindCad property status of this best fit alignment object.
ID | Read/Write: Id of the alignment Represents the ID of this alignment object.
InitID | Read/Write: Id of initial/basic alignment Represents the intial ID of this alignment object. The intial ID is the ID of the alignment to recall before modifying it with this alignment.
IterativeLevelAxis | Read/Write: Level Axis for Iterative Alignment Represents the level axis for an iterative alignment.
IterativeOriginAxis | Read/Write: Origin Axis for Iterative Alignment Represents the origin axis for an iterative alignment.
IterativeRotateAxis | Read/Write: Rotate Axis for Iterative Alignment Represents the rotate axis for an iterative alignment.
MachineToPartMatrix | Read Only: Returns a DmisMatrix object representing the machine to part matrix for the alignment Represents the matrix used to transform points between the machine and part alignment systems.
MeasAllFeat | Read/Write: Measure all features once setting for iterative alignment Represents the "Measure All Features" property of this iterative alignment object.
MeasAllFeatAlways | Read/Write: Measure All Features Always setting for iterative alignments Represents the "Measure All Features Always" property of this iterative alignment object.
NumInputs | Read Only: Number of inputs for BF3D, BF2D, or Iterative Alignments Returns the number of inputs to this alignment object. Read-only Long.
Offset | Read/Write: Alignment offset value Represents the offset property of this offset alignment object.
Parent | Read Only: Returns parent command object Returns the parent Command object. Read-only.
PointTolerance | Read/Write: Point Tolerance value for BF3D, BF2D, or Iterative alignments Represents the "Point Tolerance" property of this alignment object.
RepierceCad | Read/Write: Repierce Cad setting for Iterative Alignments Represents whether or not to repierce the cad model during the execution of this iterative alignment object.
UseBodyAxis | Read/Write: Use body axis setting for Iterative Alignments Represents whether or not to use the "Body Axis” method during the calculation of this iterative alignment object.
Workplane | Read/Write: Workplane setting for BF2D and Iterative Alignments Represents the workplane of this alignment object. It can take the values PCD_XPLUS, PCD_XMINUS, PCD_YPLUS, PCD_YMINUS, PCD_ZPLUS, and PCD_ZMINUS.

# See Also

AlignCmnd Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.