PC-Dmis 2010 MR2 Object Library | Send comments on this topic. | See Object Hierarchy Chart
SetScanParams Method
See Also

Collapse All Expand All

incr
  Increment value for LINE, BODY, and CUTAXIS scan techniques. Optional.

AXIS
  Axis for BODY and CUTAXIS scan techniques. PCD_XAXIS, PCD_YAXIS, PCD_ZAXIS. Optional.

max_incr
  For VARIABLE scan techniques. Optional.

min_incr
  For VARIABLE scan techniques. Optional.

MAX_ANGLE
  For VARIABLE scan techniques. Optional.

MIN_ANGLE
  For VARIABLE scan techniques. Optional.

delta
  Distance delta for FIXED_DELTA scans, time delta for VARIABLE_DELTA and TIME_DELTA scans. Optional.

DISTANCE
  Drop point distance for VARIABLE_DELTA scan, distance for CUTAXIS scan. Optional.

incr2
  Increment value in second direction for a patch scan. Optional.

axis2
  Second axis value for a patch scan (BODY scan technique only). Optional.

surf_thickness
  Surface thickness used to offset centroid calculation if necessary. Optional.

# Description

Sets scan parameters (used in StartScan block)

# Syntax

Visual Basic

    Public Sub SetScanParams( _
       ByVal incr As Double, _
       ByVal AXIS As PAXISTYPE, _
       ByVal max_incr As Double, _
       ByVal min_incr As Double, _
       ByVal MAX_ANGLE As Double, _
       ByVal MIN_ANGLE As Double, _
       ByVal delta As Double, _
       ByVal DISTANCE As Double, _
       ByVal incr2 As Double, _
       ByVal axis2 As PAXISTYPE, _
       ByVal surf_thickness As Double _
    )

# Parameters

incr
  Increment value for LINE, BODY, and CUTAXIS scan techniques. Optional.
AXIS

  Value | Description
  --- | ---
  PCD_ZAXIS |
  PCD_XAXIS |
  PCD_YAXIS |

  Axis for BODY and CUTAXIS scan techniques. PCD_XAXIS, PCD_YAXIS, PCD_ZAXIS. Optional.
max_incr
  For VARIABLE scan techniques. Optional.
min_incr
  For VARIABLE scan techniques. Optional.
MAX_ANGLE
  For VARIABLE scan techniques. Optional.
MIN_ANGLE
  For VARIABLE scan techniques. Optional.
delta
  Distance delta for FIXED_DELTA scans, time delta for VARIABLE_DELTA and TIME_DELTA scans. Optional.
DISTANCE
  Drop point distance for VARIABLE_DELTA scan, distance for CUTAXIS scan. Optional.
incr2
  Increment value in second direction for a patch scan. Optional.
axis2

  Value | Description
  --- | ---
  PCD_ZAXIS |
  PCD_XAXIS |
  PCD_YAXIS |

  Second axis value for a patch scan (BODY scan technique only). Optional.
surf_thickness
  Surface thickness used to offset centroid calculation if necessary. Optional.

# See Also

OldBasic Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.